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Guide Specification

 Section 12 34 00
Manufactured Plastic Cabinets


SECTION 12 35 00
WALL-MOUNTED [VANITIES] [COUNTERS]
EZ Frame by DeSavino & Sons provides a simple, pre-engineered solution for wall-mounted vanities and counters. Wall mounting simplifies floor maintenance and makes it easier to meet Americans with Disabilities Act (ADA) requirements for accessible lavatories. Excerpts from ADA Architectural Guidelines are shown at the end of this document for your reference.

SPECIFICATION COORDINATION: This document is available in word processing format at www.desavino.com/ez-frame-ada-vanity. Turn on HIDDEN TEXT to view or print specifier notes. Edit to include only requirements pertinent to Project. Edit to use either “vanity” or “counter” throughout.

DRAWING COORDINATION: Show locations and size of vanities or counters, height of countertop, lavatory locations, and clearance requirements for barrier-free access. Suggested details of accessibility guidelines can be downloaded from our website.

Coordinate use of “vanity” or “counter” with terminology used in specifications.

TECHNICAL ASSISTANCE: DeSavino & Sons

Phone +1 (570) 383-3988, email contact@desavino.com, internet www.desavino.com.

PART 1 -  GENERAL
1.1 Summary

A. Section Includes: 
1. Supports for wall-mounted [vanities] [counters].

2. [Countertop.]

Countertops: If specified in this section, retain in paragraph above. If specified in another section, retain in paragraph below.
B. Related Requirements: 

Edit following according to project requirements.

1. [Blocking.]

2. [Joint sealers.]

3. [Countertops.]

4. [Toilet Room Accessories: Templates for locations of countertop cutouts.]

5. [Plumbing Fixtures, Faucets, and Trim: Templates for locations of countertop cutouts.]

Edit following to include only references used in project specification.

1.2 REFERENCES

A. [ADA –2010 ADA Standards for Accessible Design.]

B. [ANSI A208.2 – Medium Density Fiberboard (MDF) for Interior Applications.]

C. [ASTM D638 - Tensile Properties of Plastics.]

D. [NEMA LD-3 – High Pressure Decorative Laminates Standard.]
1.3 SUBMITTALS
A. Product Data: Submit product data sheet, engineering test report, and installation instructions.

B. Shop Drawings: Indicate sizes, materials, and colors for each [vanity] [counter] configuration.

C. Samples: Submit [two] [________] samples of side panel [and countertop] materials. 

1.4 QUALITY ASSURANCE
Mock-up is not necessary for typical projects. However hotels and similar projects may require a mock-up of an entire bathroom.
A. [Mock-Ups: Install as specified in [_______________].]

1.5 DELIVERY, STORAGE, AND HANDLING

A. Comply with manufacturer’s instructions. 

PART 2 -  PRODUCTS
2.1 manufactureR

A. Provide EZ Frame by DeSavino & Sons; phone +1 570-383-3988, url www.desavino.com, email, contact@desavino.com.

B. Substitutions: None allowed.

Select above or below. Selecting below will require the architect to spend additional time reviewing substitution request.

C. Substitutions: Submit substitution request in accordance with Division 01 requirements. Submittal request shall include:

1. Documentation that proposed manufacturer has not less than five years experience manufacturing wall-mounted [vanities] [counters].

2. Proposed manufacturer’s product literature, typical details, and installation instructions.

3. Test reports demonstrating structural capacity. 
2.2 Performance Criteria

Accessibility: Excerpts from ADA, at end of guide specification, are for general guidance only. Consult other applicable regulations and authorities having jurisdiction. Indicate vanity and counter clearance requirements on Drawings.
A. Design: 

1. [Accessibility: Comply with dimensions and clearance requirements shown on Drawings.]

2. Locate side panels and intermediate brackets with consideration for location of lavatories.

DeSavino & Sons has tested vanities or counters that project 24 inches from wall. If vanity or counter projects further than 24 inches, contact us before specifying.

B. Structural Capacity:

1. [Vanity] [Counter] assemblage of horizontal frame, side panel, and intermediate bracket shall resist 85 psf (4086 N/m²) without deflection greater than 1/8 inch (3.175 mm). 

2. Provide blocking in, or reinforcement of, wall to resist inward, outward, and vertical reactions due to fully loaded [vanity] [counter].

C. Horizontal Frame: Fabricate from extruded aluminum with clear anodized finish.

Select panel materials from below. DeSavino and Sons can provide or match most commercially available panel materials and finishes.

D. Side Panels and Intermediate Brackets:

1.  [High Density Polyethylene (HDPE):

a. Product:

1) Water Absorption: 0.01 percent maximum, ASTM D570.

2) Tensile Strength: 3600 psi minimum, ASTM D638.

b. Color: [[Dolphin Grey] [Glacier Grey] [Sandshade] [Seafoam] [White-White] by Laminations, Inc.] [[_____________] color manufactured by [______________].] [As shown on Room Finish Schedule.] [Match toilet partitions.]]

2. [Plastic Laminate:

a. Core: MDF complying with ANSI 
A208.2 Grade MR10 with no added urea formaldehyde.

b. Exposed Laminate:

1) NEMA LD-3, [General-Purpose Grade (HGS).] [Vertical-surface grade (VGP).]

2) Color and Pattern: [_____________] manufactured by [______________.] [As shown on Room Finish Schedule.] [Match toilet partitions.]

c. Non-Exposed Laminate: Backer grade balancing sheet.]]

d. Adhesive: Low-VOC type.

3. [Solid Surfacing: 

a. Product: [Avonite by Aristech Surfaces,] [Corian by DuPont,] [HI-MACS by LG,] [or] [________].

b. Color: [_____________.] [As shown on Room Finish Schedule.]

FRONTS AND BOTTOMS: DeSavino can furnish vanities and counters with or without fronts and bottoms to meet a variety of conditions:

Basic: Neither fronts nor bottoms.

Utility: No fronts. Bottoms provides shelf for lightweight storage.

Commercial: Fronts satisfy ADA requirements for exposed pipes No bottoms.

Security: Fronts satisfy ADA requirements for exposed pipes. Bottoms impede use of vanity or counter to conceal contraband. Specify tamper resistant attachment or key and lock. Ventilation may be required to reduce potential for moist, moldy conditions within confined space.

E. Front (Plumbing Screens):

a. Material: Match Side Panels.

b. Attachment: Concealed fittings for push-on/pull-off installation [and [tamper-resistant fasteners.] [lock and key. [Key all locks alike.] [Provide [two] [____] keys.]]

F. Bottom:

1. [None required.]

2. [Shelf:

a. Material: Match Side Panels.

b. Construction: Shelf shall not sag in excess of 3/32-inch when loaded with 25 plf.]

3. [Security Closure: 

a. Core: MDF complying with ANSI 
A208.2 Grade MR10 with no added urea formaldehyde.

b. Laminate: NEMA LD-3 backer grade.

c. Attachment: Tamper-resistant fasteners. 

d. Ventilation of Enclosed Space: [________________].]

Delete following if countertops are specified in another section or edit as required. DeSavino will be glad to supply countertops for projects within reasonable shipping distance from our factory. 

G. Countertops [and Backsplashes]:

1. Material:

a. Solid Surfacing: [_____________] color by [______________.] [As shown on Room Finish Schedule.]

b. Quartz Surfacing: [_____________] color by [______________.] [As shown on Room Finish Schedule.]

c. Granite: [_____________________] with [_________________] finish.

2. Edges: [Eased] [Round over] [As shown on Drawings.] 

3. Attachment Devices.

Adhesives may be required for long countertops.

4. [Adhesives: Low-VOC type compatible with countertop material.] 

Use following if joint sealer at back of countertop is not specified in another section.

5. [Joint Sealer: [Translucent] [White] USDA-compliant silicone that will not stain countertop material.]

H. Fasteners: Corrosion-resistant types as required for conditions of use.
PART 3 -  EXECUTION

3.1 Examination

A. Verify that wall has adequate blocking or reinforcing. 

3.2 installation

A. Install in accordance with manufacturer’s instructions.

B. [Apply joint sealer where countertop [and backsplash] abuts walls adjacent surfaces.]

3.3 Close-out

A. [Provide keys to Owner.]
END OF SECTION

EZ Frame is trademark of DeSavino & Sons. ©2015 by DeSavino & Sons. Qualified design and construction professionals may copy for preparation of construction specifications or purchase orders. Issued August 2015; contact DeSavino & Sons for current information.
ADA GUIDELINES
The following excerpts from 2010 ADA Standards for Accessible Design (US Department of Justice, September 15, 2010) are for general guidance only. 

Consult other applicable regulations and authorities having jurisdiction. Show vanity and counter clearance requirements on project drawings.

306.2 Toe Clearance.

306.2.1 General. Space under an element between the finish floor or ground and 9 inches (230 mm) above the finish floor or ground shall be considered toe clearance and shall comply with 306.2. 

306.2.2 Maximum Depth. Toe clearance shall extend 25 inches (635 mm) maximum under an element. 

306.2.3 Minimum Required Depth. Where toe clearance is required at an element as part of a clear floor space, the toe clearance shall extend 17 inches (430 mm) minimum under the element. 

306.2.4 Additional Clearance. Space extending greater than 6 inches (150 mm) beyond the available knee clearance at 9 inches (230 mm) above the finish floor or ground shall not be considered toe clearance. 

306.2.5 Width. Toe clearance shall be 30 inches (760 mm) wide minimum. 

306.3 Knee Clearance. 

306.3.1 General. Space under an element between 9 inches (230 mm) and 27 inches (685 mm) above the finish floor or ground shall be considered knee clearance and shall comply with 306.3.

306.3.2 Maximum Depth. Knee clearance shall extend 25 inches (635 mm) maximum under an element at 9 inches (230 mm) above the finish floor or ground. 

306.3.3 Minimum Required Depth. Where knee clearance is required under an element as part of a clear floor space, the knee clearance shall be 11 inches (280 mm) deep minimum at 9 inches (230 mm) above the finish floor or ground, and 8 inches (205 mm) deep minimum at 27 inches (685 mm) above the finish floor or ground.

306.3.4 Clearance Reduction. Between 9 inches (230 mm) and 27 inches (685 mm) above the finish floor or ground, the knee clearance shall be permitted to reduce at a rate of 1 inch (25 mm) in depth for each 6 inches (150 mm) in height. 

306.3.5 Width. Knee clearance shall be 30 inches (760 mm) wide minimum. 

606 Lavatories and Sinks 

606.1 General. Lavatories and sinks shall comply with 606. 

606.2 Clear Floor Space. A clear floor space complying with 305, positioned for a forward approach, and knee and toe clearance complying with 306 shall be provided. 

EXCEPTIONS: 1. A parallel approach complying with 305 shall be permitted to a kitchen sink in a space where a cook top or conventional range is not provided and to wet bars. 

2. A lavatory in a toilet room or bathing facility for a single occupant accessed only through a private office and not for common use or public use shall not be required to provide knee and toe clearance complying with 306.
3. In residential dwelling units, cabinetry shall be permitted under lavatories and kitchen sinks provided that all of the following conditions are met: 

(a) the cabinetry can be removed without removal or replacement of the fixture; (b) the finish floor extends under the cabinetry; and (c) the walls behind and surrounding the cabinetry are finished. 

4. A knee clearance of 24 inches (610 mm) minimum above the finish floor or ground shall be permitted at lavatories and sinks used primarily by children 6 through 12 years where the rim or counter surface is 31 inches (785 mm) maximum above the finish floor or ground. 

5. A parallel approach complying with 305 shall be permitted to lavatories and sinks used primarily by children 5 years and younger. 

6. The dip of the overflow shall not be considered in determining knee and toe clearances. 

7. No more than one bowl of a multi-bowl sink shall be required to provide knee and toe clearance complying with 306. 

606.3 Height. Lavatories and sinks shall be installed with the front of the higher of the rim or counter surface 34 inches (865 mm) maximum above the finish floor or ground. 

EXCEPTIONS: 1. A lavatory in a toilet or bathing facility for a single occupant accessed only through a private office and not for common use or public use shall not be required to comply with 606.3.
2. In residential dwelling unit kitchens, sinks that are adjustable to variable heights, 29 inches (735 mm) minimum and 36 inches (915 mm) maximum, shall be permitted where rough-in plumbing permits connections of supply and drain pipes for sinks mounted at the height of 29 inches (735 mm).
606.4 Faucets. Controls for faucets shall comply with 309. Hand-operated metering faucets shall remain open for 10 seconds minimum.
606.5 Exposed Pipes and Surfaces. Water supply and drain pipes under lavatories and sinks shall be insulated or otherwise configured to protect against contact. There shall be no sharp or abrasive surfaces under lavatories and sinks.
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